**Doctoral School of Information and Biomedical Technologies**

**Polish Academy of Sciences (TIB PAN)**

**SUBJECT:** Development of optimal lung ventilation minimizing the risk of Ventilator-Induced Lung Injury (VILI)

**SUPERVISOR:** Prof. Marek Darowski, PhD, DSc, Eng.

**DESCRIPTION:** The project is focused on investigations concerning mechanisms of artificial ventilation influence on inhomogeneous, pathologically changed lungs.

The project goals are clearly cognitive expanding the current state of knowledge on the risk factors of Ventilator Induced Lung Injury (VILI), caused by: barotrauma, high driving pressure, volutrauma, atelectasis, biotrauma and ergotrauma. VILI is the worst side effect of artificial ventilation of the lungs. The results of our investigations will indicate what ventilation methods or set of ventilation parameters could be the most suitable to avoid VILI, especially in patients with lung pathology. Different criteria for minimizing the risk of VILI will be taken into account (maximum alveolar pressure, work of breathing and respiratory power).

For more than the last 7 decades, artificial ventilation of the lungs has been realized utilizing mechanical ventilators, in most cases of the respiratory system inefficiency or during surgical operations. The ventilators perform automatically by generating intermittent positive pressure at the respiratory airways, which results in continuously changed positive pressure in the alveoli. In patients with lungs pathology or/and in cases of improperly adjusted ventilation parameters like too high inspiratory pressure or tidal volume the so-called Ventilator–Induced Lung Injury (VILI) may arise, that is a bad, serious side-effect of positive pressure ventilation. Lungs have viscoelastic properties so pulmonary stress and strain resulting in VILI depends on inspiratory pressure and its rate that is proportional to inspiratory flow. It implies that inspiratory ventilation power as a product of inspiratory pressure and flow, delivered to the lungs during inspiration is a good index of the risk of VILI. So, it was assumed in the project that the optimal ventilation method is the method to deliver a requested tidal volume to the lungs with a minimum inspiratory power. Thus, the research objectives in the project are the development of the optimal lung ventilation method minimizing the risk of VILI and the assessment of the efficacy of optimal lung ventilation on a model of pathologically changed lungs. Clinical investigations are expensive, time-consuming and many patients for investigations are needed to obtain statistically proven results of studies. Besides, such institutional authorities like European Commission or the US Food and Drug Administration encourage the researcher to diminish the number of animal experiments and replace them with in silico studies, especially in a preclinical phase. Contrary to clinical investigations, modelling of a ventilator-lungs system and usage of simulation to study their interaction is cheap, saves time and generally is easy to perform for experienced investigators equipped with proper experimental tools. It is also very important that studies on virtual patients like lung models are devoid of ethical issues. To achieve the project objectives the simulation investigation will be performed on the hybrid (pneumatic–computer) simulator of the hybrid respiratory system (HRS) developed in the IBBE PAS that enables to connect of a mechanical ventilator pump with a computer model of lungs inserted in the simulator, using impedance transformers. The project result will be to find such inspiratory pressure and flow patterns to assure the minimization of mechanical power during lung ventilation and keeping it on a constant minimal level during inspiration. The results of the project will give new information to researchers, physicians and engineers working on the automation of ventilation therapy with the aim to improve its outcomes and speed up scientific investigations in this field by promoting the use of in silico simulation for ventilation strategy optimization. The method of investigation proposed in the project consists of ventilation of the lungs model that is a part of the hybrid respiratory simulator (HRS), employing an arbitrary ventilation pump (AVP) generating intermittent positive pressure of changeable patterns. As far as the risk of VILI is concerned, a potentially safe level of applied ventilation power for patients is not known up to now. So, the minimum value of ventilation power will be traced in the simulation study automatically through so-called an extreme controller.

Thanks to the unique features of the HRS-AVP system, an analysis of the possibility of test database generation will be carried out to assess the AI applicability for lung ventilation diagnostics. AI usage in cases of various lung pathologies and under conditions of limited availability of measurement data would be of great importance.

**BIBLIOGRAPHY:**

1. Tehrani FT. The Origin of Adaptive Support Ventilation. The International Journal of Artificial Organs. 2005;28(10):1051-1052. doi:10.1177/039139880502801013
2. Belliato M, Palo A, Pasero D, Iotti GA, Mojoli F, Braschi A. Evaluation of adaptive support ventilation in paralysed patients and in a physical lung model. Int J Artif Organs. 2004 Aug;27(8):709-16. doi: 10.1177/039139880402700809.
3. Santos Raquel S., de A. Maia Ligia, Oliveira M.V, et al.. Biologic Impact of Mechanical Power at High and Low Tidal Volumes in Experimental Mild Acute Respiratory Distress Syndrome. Anesthesiology 2018;128:1193–1206 doi: https://doi.org/10.1097/ALN.0000000000002143
4. Dreyfuss D, Saumon G. High inflation pressure pulmonary edema. Respective effects of high airway pressure, high tidal volume, and positive end-expiratory pressure. *The American review of respiratory disease* vol. 137,5 (1988): 1159-64. doi:10.1164/ajrccm/137.5.1159
5. Serpa Neto, A., Deliberato, R.O., Johnson, A.E.W. et al*.* Mechanical power of ventilation is associated with mortality in critically ill patients: an analysis of patients in two observational cohorts. *Intensive Care Med* 44,1914–1922 (2018).
6. Silva P.L., Ball, L., Rocco, P.R.M. et al. Power to mechanical power to minimize ventilator-induced lung injury? ICMx 7, 38 (2019). <https://doi.org/10.1186/s40635-019-0243-4>
7. Marini JJ, Rocco PRM. Which component of mechanical power is most important in causing VILI?. *Crit Care* **24,** 39 (2020). <https://doi.org/10.1186/s13054-020-2747-4>
8. Hong ., Chen L, Pan Q, et al. Individualized Mechanical power-based ventilation strategy for acute respiratory failure formalized by finite mixture modeling and dynamic treatment regimen, EClinicalMedicine 2021:36. <https://doi.org/10.1016/j.eclinm.2021.100898>.
9. Agarwal R, Srinivasan A, Aggarwal AN, Gupta D. Adaptive support ventilation for complete ventilatory support in acute respiratory distress syndrome: a pilot, randomized controlled trial. Respirology 2013 Oct;18(7):1108-15; doi: 10.1111/resp.12126.
10. Tiller NB, Campbell IG, Romer LM. Mechanical-ventilatory responses to peak and ventilation-matched upper- versus lower-body exercise in normal subjects. Exp Physiol. 2019 Jun;104(6):920-931; doi: 10.1113/EP087648. Epub 2019 Apr 15.
11. Becher T., Adelmeier, A., Frerichs I. *et al.* Adaptive mechanical ventilation with automated minimization of mechanical power - a pilot randomized cross-over study. *Crit Care* **23,** 338 (2019). <https://doi.org/10.1186/s13054-019-2610-7>
12. Divo M.J., De Pietro M.R., Horton J.R., Maguire C.A., Celli B.R. Metabolic and cardiorespiratory effects of decreasing lung hyperinflation with budesonide/formoterol in COPD: a randomized, double-crossover, placebo-controlled, multicenter trial. *Respir Res* 2020 Jan 20;21(1):26. doi: 10.1186/s12931-020-1288-3.
13. Tsuboi N, Tsuboi K, Nosaka N,et al. The Ventilatory Strategy to Minimize Expiratory Flow Rate in Ventilated Patients with Chronic Obstructive Pulmonary Disease. Int J Chron Obstruct Pulmon Dis. 2021;16:301-304. <https://doi.org/10.2147/COPD.S296343>.
14. Liaqat A, Mason M, Foster BJ, Kulkarni S, Barlas A, Farooq AM, Patak P., Liaqat H, Basso RG, Zaman MS, Pau D. Evidence-Based Mechanical Ventilatory Strategies in ARDS. *J Clin Med* 2022, 11, 319. <https://doi.org/10.3390/jcm11020319>.
15. Siegel MD, Hyzy RC. Ventilator management strategies for adults with acute respiratory distress syndrome. UpToDate 2022. <https://www.uptodate.com/contents/ventilator-management-strategies-for-adults-with-acute-respiratory-distress-syndrome>
16. Hernandez G, Pedrosa A, Ortiz R, et al. The effects of increasing effective airway diameter on weaning from mechanical ventilation in tracheostomized patients: a randomized controlled trial. Intensive Care Med. 2013 Jun;39(6):1063-70. doi: 10.1007/s00134-013-2870-7.
17. Fernández J, Miguelena D, Mulett H, Godoy J, Martinón-Torres F. Adaptive support ventilation: State of the art review. Indian J Crit Care Med. 2013;17(1):16-22. doi:10.4103/0972-5229.112149
18. Laubscher TP, Heinrichs W, Weiler N, Hartmann G, Brunner JX. An adaptive lung ventilation controller. IEEE Trans Biomed Eng. 1994 Jan;41(1):51-9. doi: 10.1109/10.277271. PMID: 8200668.
19. Cressoni M, Gotti M, Chiurazzi Ch., et al. Mechanical Power and Development of Ventilator-induced Lung Injury. Anesthesiology 2016; 124:1100–1108; doi: <https://doi.org/10.1097/ALN.0000000000001056>.
20. Huhle R, Pelosi P & de Abreu MG. Variable ventilation from bench to bedside. *Crit Care* 20**,** 62 (2016). <https://doi.org/10.1186/s13054-016-1216-6>
21. van der Staay M, Chatburn RL. Advanced modes of mechanical ventilation and optimal targeting schemes. *ICMx* 2018:**6:**30. <https://doi.org/10.1186/s40635-018-0195-0>
22. Gattinoni L, Gattarello S, Steinberg I, et al. COVID-19 pneumonia: pathophysiology and management European Respiratory Review 2021:30(162):210138. DOI: 10.1183/16000617.0138-2021
23. German Physician Explains His Alternative Ventilation Strategy for COVID-19 – Medscape – Apr 28, 2020. Available from: <https://www.medscape.com/viewarticle/929609?src=soc_fb_200501_mscpedt_news_mdscp_ventilator&faf=1>
24. Titus A, Sanghavi D. Adaptive Support Ventilation. [Updated 2022 Apr 14]. In: StatPearls [Internet]. Treasure Island (FL): StatPearls Publishing; 2022 Available from: <https://www.ncbi.nlm.nih.gov/books/NBK560652/>
25. Depta F, Torok P, Reeves V, Gentile M. Programmed Multi-Level Ventilation: A Strategy for Ventilating Non-Homogenous Lungs. Med Devices (Auckl). 2021:21;14:277-285; doi: 10.2147/MDER.S329352.
26. Candik P, Kolesar A, Nosal M, et al. (2019) Use of Programmed Multilevel Ventilation as a Superior Method for Lung Recruitment in Heart Surgery. *Int J Crit Care Emerg Med* 2019;5:067; doi.org/10.23937/2474-3674/1510067.
27. Pelosi P, Gama de Abreu M, Rocco PR. New and conventional strategies for lung recruitment in acute respiratory distress syndrome. *Crit Care* 2010;14(2):210. <https://doi.org/10.1186/cc8851>.
28. Stankiewicz B, Pałko KJ, Darowski M, Zieliński K, Kozarski M. A new infant hybrid respiratory simulator: preliminary evaluation based on clinical data. *Med Biol Eng Comput* 2017:55(11):1937-1948. <https://doi.org/10.1007/s11517-017-1635-9>.
29. Stankiewicz B., Mierzewska-Schmidt M., Górczyńska K., Pałko K.J., Baranowski A., Kozarski M., Darowski M. Ventilation inhomogeneity in CDH infants – a new attitude within a simulation study, *Biocybern Biomed Eng* 2021:41(4):1378-1389. <https://doi.org/10.1016/j.bbe.2021.08.002>
30. Stankiewicz B., Palko K.J., Darowski M., Kozarski M. How to ventilate preterm infants with lung compliance close to circuit compliance: real-time simulations on an infant hybrid respiratory simulator. *Medical Biol Eng. Comput* 2020:58(2):

357-372. [https://dx.doi.org/10.1007%2Fs11517-019-02089-5](https://dx.doi.org/10.1007/s11517-019-02089-5).

1. Bellman R. Dynamic programming. Princeton University Press, New Jersey 1957.
2. Darowski M. Volume controlled with self-adapting inspiratory flow pattern – a new approach to mechanical ventilation of the lungs. Biocybern Biomed Eng1995;15:5-15.
3. Stankiewicz B., Mierzewska-Schmidt M., Pałko K.J., et al. A new method of ventilation inhomogeneity assessment based on a simulation study using clinical data on congenital diaphragmatic hernia cases. Sci Rep 2022,12:22635.